file format : IDRISI Raster A.1
file title  : corine49toledo resampled
data type   : byte
file type   : binary
columns     : 2600
rows        : 1700
ref. system : utm-30n
ref. units  : m
unit dist.  : 1.0000000
min. X      : 270000.0000000
max. X      : 530000.0000000
min. Y      : 4320000.0000000
max. Y      : 4490000.0000000
pos'n error : 0.0000000
resolution  : 100.0000000
min. value  : 0
max. value  : 49
display min : 0
display max : 49
value units : unspecified
value error : unknown
flag value  : 0
flag def'n  : no data
legend cats : 44
code      1 : Continuous urban fabric
code      2 : Discontinuous urban fabric
code      3 : Industrial or commercial units
code      4 : Road and rail networks and associated land
code      5 : Port areas
code      6 : Airports
code      7 : Mineral extraction sites
code      8 : Dump sites
code      9 : Construction sites
code     10 : Green urban areas
code     11 : Sport and leisure facilities
code     12 : Non-irrigated arable land
code     13 : Permanently irrigated land
code     14 : Rice fields
code     15 : Vineyards
code     16 : Fruit trees and berry plantations
code     17 : Olive groves
code     18 : Pastures
code     19 : Annual crops associated with permanent crops
code     20 : Complex cultivation patterns
code     21 : Land principally occupied by agriculture, with significant areas o
code     22 : Agro-forestry areas
code     23 : Broad-leaved forest
code     24 : Coniferous forest
code     25 : Mixed forest
code     26 : Natural grasslands
code     27 : Moors and heathland
code     28 : Sclerophyllous vegetation
code     29 : Transitional woodland-shrub
code     30 : Beaches, dunes, sands
code     31 : Bare rocks
code     32 : Sparsely vegetated areas
code     33 : Burnt areas
code     34 : Glaciers and perpetual snow
code     35 : Inland marshes
code     36 : Peat bogs
code     37 : Salt marshes
code     38 : Salines
code     39 : Intertidal flats
code     40 : Water courses
code     41 : Water bodies
code     42 : Coastal lagoons
code     43 : Estuaries
code     44 : Sea and ocean
lineage     : This file was created by the RESAMPLE module with the command line: 
lineage     : O*C:\Documents and Settings\Administrador\Mis documentos\ArchiPablo\CursoToledo\corine49toledo.rst*C:\Documents and Settings\Administrador\Mis documentos\ArchiPablo\CursoToledo\corine49toledo100.rst*C:\Documents and Settings\Administrador\Mis documentos\ArchiPablo\CursoToledo\corimdt.cor*plane*m*1*0*270000*530000*4320000*4490000*2600*1700*1*1
lineage     : File resampled from corine49toledo
lineage     : Control points used in the transformation : 
lineage     :         Old X        Old Y        New X        New Y    Residual
lineage     : -----------------------------------------------------------------
lineage     : 300000.000000 4350000.000000 300000.000000 4350000.000000     0.000000
lineage     : 300000.000000 4450000.000000 300000.000000 4450000.000000     0.000000
lineage     : 500000.000000 4350000.000000 500000.000000 4350000.000000     0.000000
lineage     : 500000.000000 4450000.000000 500000.000000 4450000.000000     0.000000
lineage     : 400000.000000 4350000.000000 400000.000000 4350000.000000     0.000000
lineage     : 400000.000000 4450000.000000 400000.000000 4450000.000000     0.000000
lineage     : Overall RMS =     0.000000
lineage     : RMS Error is expressed in input image units. With low RMS errors, be
lineage     : careful that an adequate sample exists (eg. 2-3 times the mathematical min).
